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SECTION 1: PRODUCT AND COMPANY IDENTIFICATION
	Product identifier
	

	Chemical Name
	Mixture

	CAS No.

	Mixture

	Trade Name
	VP RACING SILICONE DETAILER

	Product Code
	EN-5829

	Relevant identified uses of the substance or mixture and uses advised against

	Identified Use(s)
	Protective coating

	Uses Advised Against
	None

	Company Identification
	Spray Products Corporation

P.O. Box 737

Norristown, PA  19404

	Telephone
	(610) 277-1010

	Fax
	(610) 277-4390

	E-Mail (competent person)
	sds@sprayproducts.com  

	Emergency telephone number
	

	Emergency Phone No.
	Transportation Emergency: CHEMTREC 24 hr. 1-800-424-9300 / 1 (703) 527-3887 (Collect calls accepted)


SECTION 2: HAZARDS IDENTIFICATION
	Classification of the substance or mixture

	OSHA HCS (29 CFR 1910.1200)
	Flam. Aerosol 1; Liquefied gas; Skin Irrit. 2; STOT SE 3; Asp. Tox. 1 

	Label elements

	Hazard Symbol
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	Signal word(s)
	DANGER

	Hazard Statement(s)
	Extremely flammable aerosol.
Contains gas under pressure; may explode if heated.
May be fatal if swallowed and enters airways.
Causes skin irritation.
May cause drowsiness or dizziness.

	Precautionary Statement(s)
	Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.
Do not spray on an open flame or other ignition source.
Do not pierce or burn, even after use.
Wash hands and exposed skin after use.
Wear protective gloves/protective clothing/eye protection/face protection.
Avoid breathing dust/fume/gas/mist/vapours/spray.
Protect from sunlight and do not expose to temperatures exceeding 50 ºC/122 ºF.

	Other hazards
	Toxic to aquatic life. Harmful to aquatic life with long lasting effects.


SECTION 3: COMPOSITION/INFORMATION ON INGREDIENTS
	Hazardous Ingredient(s)
% wt. *
CAS No.
Hazard classification
Heptane, branched, cyclic and linear
45-55
426260-76-6

Flam. Liq. 2; H225

Asp. Tox. 1; H304

Skin Irrit. 2; H315

STOT SE 3; H336

Aquatic Acute 2; H401

Aquatic Chronic 3; H412

Propane
10 - 20
74-98-6
Flam. Gas 1; H220

Liquefied gas; H280

n-Butane
10 - 25
106-97-8

Flam. Gas 1; H220

Liquefied gas; H280
Proprietary silicone polymers
7-12
Trade Secret
Not classified as dangerous for supply/use.
Fragrance
<1

Proprietary
Eye Irrit. 2; H319

 Skin Irrit. 2; H315.


	* The exact percentage withheld as a trade secret in accordance with 29 CFR 1910.1200.

Additional Information -  None



SECTION 4: FIRST AID MEASURES
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	Description of first aid measures
	

	Inhalation
	Move person to fresh air. If breathing is labored, administer oxygen. If symptoms develop, obtain medical attention.

	Skin Contact
	Wash affected skin with soap and water. If symptoms develop, obtain medical attention.

	Eye Contact
	Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. If eye irritation persists, get medical advice/attention.

	Ingestion
	Do not give anything by mouth to an unconscious person. Seek medical treatment. Do NOT induce vomiting.

	Most important symptoms and effects, both acute and delayed
	May be harmful if swallowed and enters airways.

	Indication of any immediate medical attention and special treatment needed
	IF SWALLOWED: Immediately call a POISON CENTER or doctor/physician. Do NOT induce vomiting.


SECTION 5: FIRE-FIGHTING MEASURES
	Extinguishing Media
	

	 -Suitable Extinguishing Media
	Extinguish with carbon dioxide, dry chemical, foam or water spray.

	 -Unsuitable Extinguishing Media
	Do not use water jet.

	Special hazards arising from the substance or mixture
	Highly flammable vapor (flash point below 23°C).

	Advice for fire-fighters
	A self contained breathing apparatus and suitable protective clothing should be worn in fire conditions. Keep containers cool by spraying with water if exposed to fire.


SECTION 6: ACCIDENTAL RELEASE MEASURES
	Personal precautions, protective equipment and emergency procedures
	Keep away from heat/sparks/open flames/hot surfaces. – No smoking. Avoid contact with skin and eyes. Avoid breathing gas/spray.

	Environmental precautions
	Prevent liquid entering sewers, basements and work pits.

	Methods and material for containment and cleaning up
	Cover spills with inert absorbent material. Transfer to a container for disposal or recovery.

	Reference to other sections
	None

	Additional Information
	None


SECTION 7: HANDLING AND STORAGE
	Precautions for safe handling
	Keep away from heat/sparks/open flames/hot surfaces. – No smoking. Avoid contact with skin and eyes. Use product in a well-ventilated area only. Avoid breathing gas/spray.

	Conditions for safe storage, including any incompatibilities
	

	 -Storage temperature 
	Keep in a cool, well ventilated place. Store at temperatures not exceeding 50 °C / 122 °F.

	 -Incompatible materials
	This product should be stored away from sources of strong heat or oxidizing chemicals.


	Specific end use(s)
	Protective coating


SECTION 8: EXPOSURE CONTROLS/PERSONAL PROTECTION              

	Occupational Exposure Limits
	

	SUBSTANCE.
CAS No.
(8hr TWA)
(STEL)
Note:
PEL

(OSHA)
TLV (ACGIH)
PEL

(OSHA)
TLV (ACGIH)
Propane

74-98-6

1000 ppm

Aspyx.#

-----

-----

#

Heptane, branched, cyclic and linear

426260-76-6
500 ppm*
1500 mg/m3
-----

-----

*n-heptane

n-Butane

106-97-8
600 ppm

250 ppm

750 ppm

-----

 ^NIC = Notice of Intended Changes (ACGIH®); #Assure minimum oxygen content

	Recommended monitoring method
	NIOSH 1500 (hydrocarbons, B.P. 36 - 126 ºC)

	Exposure controls
	

	Appropriate engineering controls
	Provide adequate ventilation to ensure that the occupational exposure limit is not exceeded.

	Personal protection equipment
	

	
	Eye/face protection
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	Wear protective eyewear (goggles, face shield, or safety glasses).

	
	Skin protection (Hand protection/ Other)
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	Wear suitable gloves if prolonged skin contact is likely (Butyl rubber). Check with protective equipment manufacturer's data. 

	
	Respiratory protection
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	Normally no personal respiratory protection is necessary. In case of insufficient ventilation, wear suitable respiratory equipment. Check with protective equipment manufacturer's data.

	
	Thermal hazards
	Not normally required. Use gloves with insulation for thermal protection, when needed.


	Environmental Exposure Controls
	Avoid release to the environment.


SECTION 9: PHYSICAL AND CHEMICAL PROPERTIES
	Information on basic physical and chemical properties

	Appearance 
	Aerosol spray

	Color.
	Not available

	Odor
	Not available

	Odor Threshold (ppm)
	Not available

	pH (Value)
	Not available

	Melting Point (°C) / Freezing Point (°C)
	Not available

	Boiling point/boiling range (°C):
	Not available

	Flash Point (°C)
	-104 (Propane)

	Evaporation Rate
	Not available

	Flammability (solid, gas)
	Flammable aerosol

	Explosive Limit Ranges
	2.1% - 9.5% v/v (Propane)

	Vapor pressure (Pascal)
	ca. 95 x 104 (Propane)

	Vapor Density (Air=1)
	ca. 1.56 @ 0 ºC (Propane)

	Density (g/ml)
	Not available

	Solubility (Water)
	Not available

	Solubility (Other)
	Not available

	Partition Coefficient (n-Octanol/water)
	Not available

	Auto Ignition Point  (°C)
	Not available

	Decomposition Temperature (°C)
	Not available

	Kinematic Viscosity (cSt)
	<20.5 @ 40 °C

	Explosive properties
	Not explosive.

	Oxidizing properties
	Not oxidizing.

	Other information
	Not available


SECTION 10: STABILITY AND REACTIVITY
	Reactivity
	Stable under normal conditions.

	Chemical stability
	Stable.

	Possibility of hazardous reactions
	None anticipated.

	Conditions to avoid
	Avoid contact with heat and ignition sources.

	Incompatible materials
	Strong oxidizing agents

	Hazardous decomposition product(s)
	Carbon monoxide, Carbon dioxide, Acrid smoke


SECTION 11: TOXICOLOGICAL INFORMATION
Exposure routes: Inhalation, Skin Contact, Eye Contact
	Heptane, branched, cyclic and linear (CAS# 426260-76-6) - By analogy with similar materials:

	Acute toxicity
	Oral: LD50 >5 g/kg-bw

Dermal: LD50 >2 g/kg-bw

Inhalation: LC50 = 65 - 103 mg/L (Vapor), 4-hr. rat

May cause drowsiness or dizziness.
May be fatal if swallowed and enters airways.

	Irritation/Corrosivity
	Causes skin irritation. Repeated exposure may cause skin dryness or cracking. May cause eye irritation.

	Sensitization
	It is not a skin sensitizer.

	Repeated dose toxicity
	NOAEC: 12350 mg/m3 (2 yr, inhal., rat, Systemic effects)

LOAEC: 1650 mg/m3 (2 hr, inhal., rat, CNS effects)

May cause drowsiness or dizziness.

	Carcinogenicity
	No data. It is unlikely to present a carcinogenic hazard to man.

	NTP

IARC

ACGIH

OSHA

NIOSH
No.
No.
No.
No.
No.


	Mutagenicity
	There is no evidence of mutagenic potential.

	Reproductive toxicity
	Not available

	Propane (CAS# 74-98-6):

	Acute toxicity
	Inhalation: LC50 = 1237 mg/L (2-hr, mouse, gas)

	Irritation/Corrosivity
	No evidence of irritant effects from normal handling and use.

	Sensitisation
	It is not a skin sensitiser.

	Repeated dose toxicity
	NOAEC: >19678 mg/m3 (28-day, rat, Systemic effects)

LOAEC: 21641 mg/m3 (28-day, rat, effects: Body weight)

	Carcinogenicity
	No data. It is unlikely to present a carcinogenic hazard to man.

	NTP

IARC

ACGIH

OSHA

NIOSH
No.
No.
No.
No.
No.


	Mutagenicity
	There is no evidence of mutagenic potential.

	Reproductive toxicity
	None anticipated


SECTION 12: ECOLOGICAL INFORMATION
	Ecotoxicity
	

	Heptane, branched, cyclic and linear (CAS# 426260-76-6) - By analogy with similar materials:

	Short term
	LL50 (96 hour): >13.4 mg/L (Oncorhynchus mykiss)

EL50 (48 hour): 3 mg/l (Daphnia magna, mobility)

EC50 (96 hour): 13 mg/l (Pseudokirchnerella subcapitata)

	Long Term
	NOELR (28 days) 1.5 mg/l (Fish) QSAR

LOEC (21 days): 0.32 mg/l (Daphnia magna)

NOEL (96 hour) 6.3 mg/l (Algae)

	Propane (CAS# 74-98-6):

	Short term (estimate)
	LC50 (96 hour): 27.98 mg/L (fish)

LC50 (48 hour): 14.22 mg/L (crustacea)

EC50 (96 hour): 7.71 mg/L (algae)

	Long Term
	No data.

	Persistence and degradability
	Readily biodegradable.

	Bioaccumulative potential

	The product has no potential for bioaccumulation.

	Mobility in soil
	Not available.

	Results of PBT and vPvB assessment
	Not classified as PBT or vPvB.

	Other adverse effects
	None known.


SECTION 13: DISPOSAL CONSIDERATIONS
	Waste treatment methods
	Disposal should be in accordance with local, state or national legislation. Consult an accredited waste disposal contractor or the local authority for advice.


SECTION 14: TRANSPORT INFORMATION
	
	U.S. DOT
	Sea transport
(IMDG)
	Air transport (ICAO/IATA)

	UN number
	1950
	1950
	1950

	Proper Shipping Name
	Aerosols, flammable
	Aerosols, flammable
	Aerosols, flammable

	Transport hazard class(es)
	2.1
	2.1
	2.1

	Packing group
	Not applicable
	Not applicable
	Not applicable

	Environmental hazards
	None assigned
	None assigned
	None assigned

	Special precautions for user
	None assigned
	None assigned
	None assigned

	Transport in bulk according to Annex II of MARPOL73/78 and the IBC Code: Not applicable


SECTION 15: REGULATORY INFORMATION
	Safety, health and environmental regulations/legislation specific for the substance or mixture:

	TSCA (Toxic Substance Control Act) - Inventory Status: All components listed or polymer exempt.

	Designated Hazardous Substances and Reportable Quantities (40 CFR 302.4):

	
	Chemical Name
	CAS No.
	Typical %wt.
	RQ (Pounds)

	
	                 None
	------
	------
	

	SARA 311/312 - Hazard Categories: See SECTION 2: HAZARDS IDENTIFICATION

	
	

	SARA 313 - Toxic Chemicals (40 CFR 372): 

	Chemical Name
	CAS No.
	Typical %wt.

	None
	----
	----

	SARA 302 - Extremely Hazardous Substances(40 CFR 355):

	
	Chemical Name
	CAS No.
	Typical %wt.
	TPQ (pounds)

	
	None
	----
	----
	----

	California Proposition 65 List:

	
	Chemical Name
	CAS No.
	Type of Toxicity

	
	None
	----
	----


SECTION 16: OTHER INFORMATION
	The following sections contain revisions or new statements: 1-16.
Date of preparation: February 19,2024

	Hazard Statement(s) 
- H220: Extremely flammable gas.
- H225: Highly flammable liquid and vapor.
- H280: Contains gas under pressure; may explode if heated.
- H304: May be fatal if swallowed and enters airways.
- H315: Causes skin irritation.
- H319: Causes serious eye irritation.
- H336: May cause drowsiness or dizziness.
- H400: Very toxic to aquatic life.
- H401: Toxic to aquatic life.
- H410: Very toxic to aquatic life with long lasting effects.
- H412: Harmful to aquatic life with long lasting effects.

	Training advice: None.


Disclaimer: We believe the statements, technical information and recommendations contained herein are reliable, but they are given without warranty or guarantee of any kind. The information contained in this document applies to this specific material as supplied. It may not be valid for this material if it is used in combination with any other materials. It is the user’s responsibility to satisfy oneself as to the suitability and completeness of this information for the user’s own particular use.
�DOCVARIABLE GMSD00056AA0136 \* MERGEFORMAT�SAFETY DATA SHEET�


�DOCVARIABLE GMSA00001AA0013 \* MERGEFORMAT�OSHA HCS (29 CFR 1910.1200)�
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