VP RACING BRAKE PARTS CLEANER 
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SECTION 1: PRODUCT AND COMPANY IDENTIFICATION
	Product identifier
	

	Chemical Name
	Mixture

	CAS No.

	Mixture

	Trade Name
	VP RACING BRAKE CLEANER

	Product Code
	EN-5831

	Relevant identified uses of the substance or mixture and uses advised against

	Identified Use(s)
	Brake cleaner

	Uses Advised Against
	None

	Company Identification
	Spray Products Corporation
P.O. Box 737

Norristown, PA  19404

	Telephone
	(610) 277-1010

	Fax
	(610) 277-4390

	E-Mail (competent person)
	sds@sprayproducts.com  

	Emergency telephone number
	

	Emergency Phone No.
	Transportation Emergency: CHEMTREC 24 hr. 1-800-424-9300 / 1 (703) 527-3887 (Collect calls accepted)


SECTION 2: HAZARDS IDENTIFICATION
	Classification of the substance or mixture

	OSHA HCS (29 CFR 1910.1200)
	Flam. Aerosol 1; Compressed dissolved gas; Acute Tox. 4; STOT SE 1 Repr. 2; STOT RE 2; Skin Irrit. 2; Eye Irrit. 2; Asp. Tox. 1
 

	Label elements

	Hazard Symbol
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	Signal word(s)
	DANGER

	Hazard Statement(s)
	Extremely flammable aerosol.
Contains gas under pressure; may explode if heated.
Harmful if swallowed. Harmful if inhaled. Harmful in contact with skin.
Causes damage to organs: Optic nerve, Central nervous system. May cause drowsiness or dizziness.
Suspected of damaging the unborn child.
May cause damage to organs through prolonged or repeated exposure: Inhalation - neuropsychological effects, auditory dysfunction and effects on colour vision. 
Causes skin irritation. Causes serious eye irritation.
Repeated exposure may cause skin dryness or cracking.
May be harmful if swallowed and enters airways.

	Precautionary Statement(s)
	Do not handle until all safety precautions have been read and understood.
Keep away from heat/sparks/open flames/hot surfaces. – No smoking.
Do not spray on an open flame or other ignition source.
Do not breathe mist/vapours/spray. 

Wash hands and exposed skin after use.
Protect from sunlight and do not expose to temperatures exceeding 50 ºC/122 ºF.
Keep out of reach of children.

	Other hazards
	None


SECTION 3: COMPOSITION/INFORMATION ON INGREDIENTS
	Hazardous Ingredient(s)
% wt. *
CAS No.
Hazard classification
Acetone

45-55
67-64-1
Flam. Liq. 2; H225

Eye Irrit. 2; H319
STOT SE 3; H336
Methanol

1-5
67-56-1
Flam. Liq. 2; H225
Acute Tox. 3; H301, H311, H331
STOT SE 1; H370 (Optic nerve, Central nervous system)
Toluene
1-5
108-88-3
Flam. Liq. 2; H225

Repr. 2; H361

Skin Irrit. 2; H315

Eye Irrit. 2; H319

Asp. Tox. 1; H304

STOT SE 3; H336

STOT RE 2; H373: Inhalation - neuropsychological effects, auditory dysfunction and effects on colour vision.

Aquatic Chronic 4; H412
Heptane, branched, cyclic and linear

30-40
426260-76-6
Flam. Liq. 2; H225

Asp. Tox. 1; H304 

Skin Irrit. 2; H315

STOT SE 3; H336

Carbon dioxide
4-10
124-38-9
Compressed dissolved gas


	Additional Information -  None

	* The exact percentage withheld as a trade secret in accordance with 29 CFR 1910.1200.


SECTION 4: FIRST AID MEASURES
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	Description of first aid measures
	

	Inhalation
	Move person to fresh air. If breathing is labored, administer oxygen. If symptoms develop, obtain medical attention.

	Skin Contact
	Wash affected skin with soap and water. If symptoms develop, obtain medical attention.

	Eye Contact
	IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. If symptoms occur obtain medical attention.

	Ingestion
	Do not give anything by mouth to an unconscious person. Seek medical treatment.

	Most important symptoms and effects, both acute and delayed
	May cause damage to organs: (Optic nerve, Central nervous system). May be harmful if swallowed and enters airways. 

	Indication of any immediate medical attention and special treatment needed
	IF SWALLOWED: Immediately call a POISON CENTER or doctor/physician. Do NOT induce vomiting.


SECTION 5: FIRE-FIGHTING MEASURES
	Extinguishing Media
	

	 -Suitable Extinguishing Media
	Extinguish with carbon dioxide, dry chemical, foam or water spray.

	 -Unsuitable Extinguishing Media
	Do not use water jet.

	Special hazards arising from the substance or mixture
	Highly flammable vapor (flash point below 23°C).

	Advice for fire-fighters
	A self contained breathing apparatus and suitable protective clothing should be worn in fire conditions. Keep containers cool by spraying with water if exposed to fire.


SECTION 6: ACCIDENTAL RELEASE MEASURES
	Personal precautions, protective equipment and emergency procedures
	Keep away from heat/sparks/open flames/hot surfaces. – No smoking. Take precautionary measures against static discharges. Avoid contact with skin and eyes. Avoid breathing vapors.

	Environmental precautions
	Prevent liquid entering sewers, basements and work pits.

	Methods and material for containment and cleaning up
	Cover spills with inert absorbent material. Transfer to a container for disposal or recovery.

	Reference to other sections
	None

	Additional Information
	None


SECTION 7: HANDLING AND STORAGE
	Precautions for safe handling
	Keep away from heat/sparks/open flames/hot surfaces. – No smoking. Avoid contact with skin and eyes. Use product in a well-ventilated area only.

	Conditions for safe storage, including any incompatibilities
	

	 -Storage temperature 
	Keep in a cool, well ventilated place. Store at temperatures not exceeding 50 °C / 122 °F.

	 -Incompatible materials
	This product should be stored away from sources of strong heat or oxidizing chemicals.


	Specific end use(s)
	Brake cleaner


SECTION 8: EXPOSURE CONTROLS/PERSONAL PROTECTION              
	Occupational Exposure Limits
	

	SUBSTANCE.
CAS No.
(8hr TWA)
(STEL)
Note:
PEL

(OSHA)
TLV (ACGIH)
PEL

(OSHA)
TLV (ACGIH)
Acetone

67-64-1
1000
500
------
750
^NIC

Methanol

67-56-1

200 ppm
200 ppm

----

250 ppm

None
Toluene
108-88-3

200
20
300*
------
*10-min. Ceiling

Heptane, branched, cylic and linear

426260-76-6
500 ppm**
1500 mg/m3
-----

-----

**n-heptane

Carbon dioxide

124-38-9
5000 ppm

30,000 ppm

^NIC = Notice of Intended Changes (ACGIH®); 

	Recommended monitoring method
	NIOSH 1300 (Ketones I); NIOSH 2000 (Methanol); NIOSH 1500 (hydrocarbons, B.P. 36 - 126 ºC) ; NIOSH 1501 (Hydrocarbons, Aromatic)

	Exposure controls
	

	Appropriate engineering controls
	Provide adequate ventilation to ensure that the occupational exposure limit is not exceeded.

	Personal protection equipment
	

	
	Eye/face protection
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	Wear protective eyewear (goggles, face shield, or safety glasses).

	
	Skin protection (Hand protection/ Other)
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	Wear suitable gloves if prolonged skin contact is likely (Nitrile rubber)

	
	Respiratory protection
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	Normally no personal respiratory protection is necessary. In case of insufficient ventilation, wear suitable respiratory equipment.

	
	Thermal hazards
	Not normally required. Use gloves with insulation for thermal protection, when needed.


	Environmental Exposure Controls
	None known


SECTION 9: PHYSICAL AND CHEMICAL PROPERTIES
	Information on basic physical and chemical properties

	Appearance 
	Liquid

	Color.
	Colorless

	Odor
	Acetone-like

	Odor Threshold (ppm)
	Not available

	pH (Value)
	Not available

	Melting Point (°C) / Freezing Point (°C)
	Not available

	Boiling point/boiling range (°C):
	56  (Acetone)

	Flash Point (°C)
	-17 (Acetone)

	Evaporation Rate
	Not available

	Flammability (solid, gas)
	Not applicable

	Explosive Limit Ranges
	2.5% - 12.8% v/v  (Acetone)

	Vapor pressure (Pascal)
	2.4 x 104  (Acetone)

	Vapor Density (Air=1)
	Not available

	Density (g/ml)
	Not available

	Solubility (Water)
	Not available

	Solubility (Other)
	Not available

	Partition Coefficient (n-Octanol/water)
	Not available

	Auto Ignition Point  (°C)
	465 (Acetone)

	Decomposition Temperature (°C)
	Not available

	Kinematic Viscosity 
	<20

	Explosive properties
	Not explosive.

	Oxidizing properties
	Not oxidizing.

	Other information
	Not available


SECTION 10: STABILITY AND REACTIVITY
	Reactivity
	Stable under normal conditions.

	Chemical stability
	Stable.

	Possibility of hazardous reactions
	None anticipated.

	Conditions to avoid
	Avoid contact with heat and ignition sources.

	Incompatible materials
	Strong oxidizing agents

	Hazardous decomposition product(s)
	Carbon monoxide, Carbon dioxide, Acrid smoke


SECTION 11: TOXICOLOGICAL INFORMATION
Exposure routes: Inhalation, Skin Contact, Eye Contact
	Information on toxicological effects

	Methanol (CAS# 67-56-1) 

	Acute toxicity *
	LD50 (oral, monkey): 7000 mg/kg-bw

LD0 (oral, rat): > 2528 mg/kg-bw

LC50 (inhal., cat, 6-hours): 43.68 mg/L

LC50 (inhal., monkey, 4-hours): 52 mg/L

Ingestion may damage the optic nerve.

May cause dizziness and drowsiness.



	Irritation
	May cause eye irritation.

	Sensitisation
	It is not a skin sensitiser.

	Repeated dose toxicity
	NOAEC (2-yr. inhal., mouse): > 1.3 mg/L

	Developmental Toxicity
	Negative. Not a specific developmental toxin.

	Toxicity for reproduction
	Negative. Not a specific reproductive toxin.

	Mutagenicity
	Negative

	Carcinogenicity

	NTP

IARC

ACGIH

OSHA

NIOSH
No.
No.
No.
No.
No.


	Other information
	* ATE (oral) = 100 mg/kg

* ATE (dermal) = 300 mg/kg

* ATE (inhalation) = 3 mg/L

	*ATE = Acute Toxicity Estimate for purposes of classification

	Acetone (CAS No. 67-64-1)

	Acute toxicity
	Oral LD50 = 5800 mg/kg (rat)
Dermal LD50 >15800 mg/kg (rabbit) 

Inhalation LC50 76 mg/L (4 hour(s)) (rat) - Vapours may cause drowsiness and dizziness.

	Irritation / Corrosivity
	Causes serious eye irritation. Repeated exposure may cause skin dryness or cracking.

	Sensitisation
	It is not a skin sensitiser.

	Repeated dose toxicity
	Oral NOAEL = 900 mg/kg/day (rat) (90-days)

Inhalation NOAEL > 19,000 ppm (rat)

	Carcinogenicity
	It is unlikely to present a carcinogenic hazard to man.

	NTP

IARC

ACGIH

OSHA

NIOSH
No.
No.
No.
No.
No.


	Mutagenicity
	Negative

	Toxicity for reproduction
	Negative

	Other information
	None known.

	
	

	Toluene (CAS No. 108-88-3)
	

	Acute toxicity

	Oral LD50 = 5580 mg/kg (rat)
Dermal LD50 >5000 mg/kg (rabbit)
Inhalation LC50 (4 hour(s)) 28.1 mg/l (rat) - Vapours may cause drowsiness and dizziness.

	Irritation / Corrosivity
	Causes serious eye irritation. Causes skin irritation.

	Sensitisation
	It is not a skin sensitiser.

	Repeated dose toxicity
	Inhalation NOAEC = 1131 mg/m3 (rat), 2 Year(s) - May cause damage to organs through prolonged or repeated exposure: neuropsychological effects, auditory dysfunction and effects on colour vision.

	Carcinogenicity
	It is unlikely to present a carcinogenic hazard to man.

	NTP

IARC

ACGIH

OSHA

NIOSH
No.
No.
No.
No.
No.


	Mutagenicity
	There is no evidence of mutagenic potential.

	Reproductive toxicity
	Suspected of damaging the unborn child. NOAEC: 2.8 mg/liter (rat)

	Heptane, branched, cylic and linear (CAS# 426260-76-6) - By analogy with similar materials:

	Acute toxicity
	Oral: LD50 >5 g/kg-bw

Dermal: LD50 >2 g/kg-bw

Inhalation: LC50 = 65 - 103 mg/L (Vapor), 4-hr. rat

May cause drowsiness or dizziness.
May be fatal if swallowed and enters airways.

	Irritation/Corrosivity
	Causes skin irritation. Repeated exposure may cause skin dryness or cracking. May cause eye irritation.

	Sensitization
	It is not a skin sensitizer.

	Repeated dose toxicity
	NOAEC: 12350 mg/m3 (2 yr, inhal., rat, Systemic effects)

LOAEC: 1650 mg/m3 (2 hr, inhal., rat, CNS effects)

May cause drowsiness or dizziness.

	Carcinogenicity
	No data. It is unlikely to present a carcinogenic hazard to man.

	NTP

IARC

ACGIH

OSHA

NIOSH
No.
No.
No.
No.
No.


	Mutagenicity
	There is no evidence of mutagenic potential.

	Reproductive toxicity
	Not available


SECTION 12: ECOLOGICAL INFORMATION
	Substances in preparations / mixtures:
	

	Toluene (CAS No. 108-88-3)
	

	Acute toxicity 
	LC50 (96 hour): 5.5 mg/l (Oncorhynchus kisutch)

EC50 (48 hour): 3.78 mg/l (Ceriodaphnia dubia)
EC50 (3 hour): 134 mg/l (Algae)

	Long Term Toxicity
	NOEC (40 days): 1.39 mg/l (Oncorhynchus kisutch)

NOEC (7 days): 0.74 mg/l (Ceriodaphnia dubia)

	Heptane, branched, cylic and linear (CAS# 426260-76-6) - By analogy with similar materials:
Short term
LL50 (96 hour): >13.4 mg/L (Oncorhynchus mykiss)EL50 (48 hour): 3 mg/l (Daphnia magna, mobility)
EC50 (96 hour): 13 mg/l (Pseudokirchnerella subcapitata)
Long Term
NOELR (28 days) 1.5 mg/l (Fish) QSAR

LOEC (21 days): 0.32 mg/l (Daphnia magna)

NOEL (96 hour) 6.3 mg/l (Algae)


	Persistence and degradability
	Readily biodegradable.

	Bioaccumulative potential

	The product has no potential for bioaccumulation.

	Mobility in soil
	Not available.

	Results of PBT and vPvB assessment
	Not classified as PBT or vPvB.

	Other adverse effects
	None known.


SECTION 13: DISPOSAL CONSIDERATIONS
	Waste treatment methods
	Disposal should be in accordance with local, state or national legislation. Consult an accredited waste disposal contractor or the local authority for advice.


SECTION 14: TRANSPORT INFORMATION
	
	U.S. DOT
	Sea transport
(IMDG)
	Air transport (ICAO/IATA)

	UN number
	1950
	1950
	1950

	Proper Shipping Name
	Aerosols, flammable
	Aerosols, flammable
	Aerosols, flammable

	Transport hazard class(es)
	2.1
	2.1
	2.1

	Packing group
	Not applicable
	Not applicable
	Not applicable

	Environmental hazards
	None assigned
	None assigned
	None assigned

	Special precautions for user
	None assigned
	None assigned
	None assigned

	Transport in bulk according to Annex II of MARPOL73/78 and the IBC Code: Not applicable


SECTION 15: REGULATORY INFORMATION
	Safety, health and environmental regulations/legislation specific for the substance or mixture:

	TSCA (Toxic Substance Control Act) - Inventory Status: All components listed or polymer exempt.

	Designated Hazardous Substances and Reportable Quantities (40 CFR 302.4):

	
	Chemical Name
	CAS No.
	Typical %wt.
	RQ (Pounds)

	
	Acetone
	67-64-1
	40 - 60
	5000

	
	Methanol
	67-56-1
	10 - 30
	5000

	
	Toluene
	108-88-3
	3 - 6
	1000

	SARA 311/312 - Hazard Categories: See SECTION 2: HAZARDS IDENTIFICATION

	
	

	SARA 313 - Toxic Chemicals (40 CFR 372): 

	Chemical Name
	CAS No.
	Typical %wt.

	Methanol
	67-56-1
	1 - 5

	Toluene
	108-88-3
	15 - 20

	SARA 302 - Extremely Hazardous Substances(40 CFR 355):

	
	Chemical Name
	CAS No.
	Typical %wt.
	TPQ (pounds)

	
	None
	----
	----
	----

	California Proposition 65 List:

	
	Chemical Name
	CAS No.
	Type of Toxicity

	
	Methanol
	67-56-1
	Developmental

	
	Toluene
	108-88-3
	Developmental, Female Reproductive


SECTION 16: OTHER INFORMATION
	The following sections contain revisions or new statements: 1-16.
Date of preparation: February 19,2024

	Hazard Statement(s) and Risk Phrases Listed in: SECTION 2:/ SECTION 3:
Hazard Statement(s)
- H225: Highly flammable liquid and vapor.
- H301: Toxic if swallowed.
- H304: May be fatal if swallowed and enters airways.
- H311: Toxic in contact with skin.
- H315: Causes skin irritation.
- H319: Causes serious eye irritation.
- H331: Toxic if inhaled.
- H336: May cause drowsiness or dizziness.
- H361: Suspected of damaging fertility or the unborn child.
- H370: Causes damage to organs. 
- H373: May cause damage to organs through prolonged or repeated exposure.

	Training advice: None.


Disclaimer: We believe the statements, technical information and recommendations contained herein are reliable, but they are given without warranty or guarantee of any kind. The information contained in this document applies to this specific material as supplied. It may not be valid for this material if it is used in combination with any other materials. It is the user’s responsibility to satisfy oneself as to the suitability and completeness of this information for the user’s own particular use.
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